{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet2"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet2","index":0,"n_rows":69,"n_cols":7,"rows_kept":69,"merged":[[0,0,0,6],[2,5,3,5],[5,5,6,5]],"flags":["formulas_cached_only"]}
["重庆中科检测技术服务有限公司仪器设备采购清单"]
["编号","仪器名称","数量","单位","关键配置","其他配置","备注"]
[1,"气相色谱仪",1,"台","150位以上自动进样器，FID,ECD,FPD检测器，电脑","带稳压电源"]
[2,"气相色谱仪",1,"台","双FID，双柱，带稳压电源，电脑"]
[3,"高效液相色谱仪",1,"台","紫外检测器和荧光检测器；带100位以上自动进样器，电脑","带稳压电源"]
[4,"气相色谱质谱仪",1,"台","自动进样器，双进样口，FID，热脱附与色谱连接可重复使用，电脑","带稳压电源"]
[5,"热脱附解吸仪",1,"台","配50根热脱附解析管"]
[6,"ICP-MS",1,"台","循环冷却机，泵，自动进样器，电脑","带稳压电源"]
[7,"原子吸收分光光度计（AAS）",1,"台","火焰，石墨炉，循环冷却水箱，空气泵，15个元素灯，自动进样器，电脑","带稳压电源"]
[8,"原子荧光光度计",1,"台","带自动进样器，电脑，5个元素灯","带稳压电源"]
[9,"离子色谱仪（IC）",1,"台","带自动进样器，电脑，淋洗液发生器，阴离子色谱柱","带稳压电源"]
[10,"紫外可见分光光度计",2,"台","1,2,3,4cm的玻璃和石英比色皿 "]
[11,"红外分光测油仪",1,"台","电脑，比色皿及架"]
[12,"旋转式蒸发仪",1,"台","真空泵，循环冷凝水"]
[13,"土壤球磨机",1,"台","玛瑙罐，玛瑙球，电动筛分机，筛子"]
[14,"微波消解仪",1,"台","赶酸器，消解罐，防护罩"]
[15,"pH计",2,"台","氟离子选择电极，饱和甘汞电极，pH电极"]
[16,"便携式多参数水质分析仪",1,"台","pH电极，电导率电极，溶解氧电极，氧化还原电极"]
[17,"立式压力蒸汽灭菌器",2,"台"]
[18,"生化培养箱",3,"台"]
[19,"恒温恒湿箱",3,"台"]
[20,"生物显微镜",1,"台"]
[21,"万分之一天平",1,"台"]
[22,"百分之一天平",1,"台"]
[23,"校准砝码",1,"套","E1级，1mg～2Kg"]
[24,"超声波清洗机",2,"台","容积30L，微电脑调节"]
[25,"隔膜真空泵",2,"台"]
[26,"高速冷冻离心机",1,"台","10mL,25mL,50mL,100mL互换组件"]
[27,"移液枪",1,"台","10-100uL"]
[28,"移液枪",3,"台","1-10ml"]
[29,"移液枪",2,"台","100-1000μl"]
[30,"数字瓶口滴定器",2,"台","25mL/50mL"]
[31,"瓶口分配器",1,"台","1-10mL可调"]
[32,"超纯水系统",1,"台"]
[33,"立式冰柜",5,"台","320L立式四层"]
[34,"立式冰箱",2,"台","200L以上"]
[35,"立式冰箱",1,"台","260L以上"]
[36,"冰箱（无霜）",1,"台","258L以上，要求带锁"]
[37,"林格曼测黑望远镜",1,"台"]
[38,"大气压力表",2,"台"]
[40,"声校准器(一级）",1,"台"]
[41,"声校准器（二级）",1,"台"]
[42,"多功能声级计（二级）",2,"台"]
[43,"多功能声级计（一级）",1,"台","频率计权，延长线，延长杆"]
[44,"热球式风速风向仪",1,"台"]
[45,"水平振荡仪 ",1,"台"]
[46,"空气压力盒",3,"台"]
[47,"水温计",3,"个"]
[48,"电热恒温干燥箱",4,"台"]
[49,"标准COD消解装置",2,"台"]
[50,"手持式电动深水采样器",1,"台"]
[51,"土壤采样器",1,"套","满足金属，有机物采样"]
[52,"冷冻干燥仪",1,"台","满足42个土壤样品同时冷冻干燥的要求"]
[53,"数显温湿度计",1,"台"]
[54,"便携式余氯总氯快速测定仪",1,"台"]
[55,"氢气发生器",1,"台","0-500ml/min，氢气纯度99.999%"]
[56,"涡旋混合仪",1,"台"]
[57,"流量压力综合校定仪",1,"台","皂膜流量计测量范围：（100～6000）ml/min；\n容积式流量计测量范围：（5.0～80.0）L/min；\n小孔口流量计测量范围：（80.0～120.0）L/min；\n大孔口流量计测量范围：（800.0～1200.0）L/min；"]
[58,"多功能蒸馏装置",1,"台","平行蒸馏6个"]
[59,"水质硫化物酸化吹气仪",1,"台","6通道"]
[60,"自动烟尘气测试仪（定电位）",3,"台","6个探头/套，二氧化硫专用烟枪2根，含可调温伴热管2根；含湿量仪器法烟枪2根；加配低浓度颗粒物烟枪4根；油烟烟枪1根及油烟滤嘴20个；沥青烟烟枪1根；硫酸雾，盐酸雾，氟化物采样器1套"]
[61,"智能双路烟气采样器",1,"台"]
[62,"智能大气综合采样器",4,"台","TSP/PM10/PM2.5切割器"]
[63,"智能四路空气采样器",1,"台"]
[64,"塞氏盘",4,"个"]
[65,"环境振动仪",1,"台","带1/3倍频带振级"]
[66,"数显温度计",1,"个","能测量J、K、T、E、R、S和N型"]
[67,"无菌操作台",1,"台","保证洁净度100级@≥0.5um(美联邦209E)"]
[null,null,102]